You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > IP Address Query 0x00E6

IP Address Query 0x00E6

SwitchKit Name

IPAddressQuery

Type

EXS API and SwitchKit API message

Description

IP Address Query 0x00E6

This message allows the host to query the IP address, subnet mask, and reset indicator for Common Channel Signaling cards, VDAC cards, and VDAC VoIP Modules.

Sent by

Host

SwitchKit Code

C Structure

typedef struct {

UBYTE Slot;

} XL_IPAddressQuery;

C Structure Response

typedef struct {

unsigned short Status;

UBYTE TLVCount;

UBYTE Data[250];

} XL_IPAddressQueryAck;

C++ Class

class XLC_IPAddressQuery : public XLC_OutboundMessage {

public:

UBYTE getSlot() const;

void setSlot(UBYTE x);

};

C++ Class Response

class XLC_IPAddressQueryAck : public XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

UBYTE getTLVCount() const;

void setTLVCount(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x000B)
3, 4 | Message Type (0x00E6) | 3, 4 | Message Type (0x00E6)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x00 - Individual AEs | 8, 9 | Status MSB, LSB
Number of AEs to follow
AE 0x01 Slot
: | Checksum | 10 | Number of TLVs
| Response continued below:
: | TLV 0x01 Module, IP Address, and Subnet Mask 0x04 Reset Indicator 0x05 Gateway IP 0x09 Ethernet Link Redundancy 0x0A Activate Ethernet Port
: | Checksum

Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.