You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > Overview

Overview

Features

The DSP Series 2 card has the following File Record/Playback functionality:

• Large Vocabulary/Disk Based Files

• Permanent File Recording (stored on an NFS server)

• Temporary Recording (stored on the card)

• Configurable Beep Tone (notifies parties that they can begin recording their voice)

• Gain/Speed Modification

• Skip Forward/Backward (in 100 ms increments)

• Silence Threshold Modification

• Conference Recording

• Pause and Resume

• Dual channel recording

• Moving temporary recordings from the card’s cache into permanent storage on a server

Supported Encoding Formats

See Encoding Formats for more information.

Configuration

See Record/Play Files.

Digital Signal Processor