0x0674 Echo Cancel NLP Type

Use this TLV in the Generic Card Configure message to set card-level parameters for Echo Cancel.

Byte | Description
0, 1 | Tag: 0x0674
2, 3 | Length: 0x0001
4 | Value [0] NLP Type This enables/disables the Non Linear Processor and, when the NLP is enabled, sets the type of Comfort Noise Generator used. 0x00 = Off 0x01 = On 0x02 = Random Noise CNG 0x03 = Hoth Noise CNG 0x04 = Maximum Suppression

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.