0x001E Generic PPL

Used in:
Route Control message
Connect With Data message

ICB Type | 0x03 (Extended Data)
ICB ID | 0x001E
Data Length (2 bytes) | Variable
Number of TLVs (2bytes) | Variable
Tag | TLV 1 Tag
Length | TLV 1 Length
Value | TLV 1 Value
: | TLV n Tag
: | TLV n Length
: | TLV n Value
TLVs | 0x11 Signaling Route Test Control Status 0x12 Signaling Route Test Control DPC 0x01 Add Virtual Card 0x000F Router Protocol ID 0x0013 Routing Method 0x0065 Physical VoIP Channel 0x0071 Virtual VoIP Channel 0x0100 RTP Payload Type (VDAC-ONE) 0x0100 RTP Payload Type (IPN Series 2) 0x0102 RTP Silence Suppression 0x0103 RTP Echo Cancellation 0x0116 Channel Service TLV 0x0117 Alerting Propagation Mode 0x0118 Companding Conversion Mode 0x011A Call Agent Mode Physical Channel ID 0x0141 Modify Connection 0x01C2 Minimum Jitter Buffer Delay 0x01C3 Maximum Jitter Buffer Delay (IPN-2 Card) 0x01C4 Adaptation Rate 0x01C7 Fax/Modem Bypass Coder Type 0x0612 Connection Type

See Information Control Block.
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.