0x53 Object Type

This AIB is generic. It can be used in any Configure and Query message introduced in Release 8.0 and above to configure and query any component. The Object Type field indicates the type of object to be configured, and the Object Instance ID field indicates the ID of the particular instance of the Object in the Object Type field.

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x53
3 | Data Length: 0x04
4 | Data[0, 1] Object Type This field indicates the type of object for which the configuration is meant. For example, to configure an SS7 Series 3 Card, the type is SS7 Stack Type. 0x0001 V.52 Interface 0x0002 SS7 Stack 0x0003 ISDN 0x0004 H323 0x0005 SINAP SS7 0x0020 IP Signaling Series 3 Card Interface 0xFFFF All object types
5, 6 | Data[2, 3] Object Instance ID (CSP Matrix Series 3 Card ID) This field addresses the particular instance of the Object listed in the Object Type field. 0xFFFF means that the Object Instance ID does not matter.

See Address Information Block.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
See Signaling System Number Seven.
See Integrated Services Digital Network.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.