0x0100 RTP Payload Type (VDAC-ONE)

Used in:
0x1E and 0x001E Generic PPL ICBs in:
Outseize Control message
Route Control message
Resource Attribute Query message
Resource Attribute Configure message

Byte | Description
0, 1 | Tag 0x0100 RTP Payload Type
2, 3 | Length 0x0001
4 | Value[0] Payload Type Basic Packet Rate 0x00 G.711 A-Law 20 ms 0x01 G.711 µ-Law (Default) 20 ms 0x02 G.726 16 Kbps 20 ms 0x03 G.726 24 Kbps 20 ms 0x04 G.726 32 Kbps 20 ms 0x05 G.726 40 Kbps 20 ms 0x06 G.727 16 Kbps 20 ms 0x07 G.727 24–16 Kbps 20 ms 0x08 G.727 24Kbps 20 ms 0x09 G.727 16–32 Kbps 20 ms 0x0A G.727 24 –32 Kbps 20 ms 0x0B G.727 32 Kbps 20 ms 0x0C G.727 16–40 Kbps 20 ms 0x0D G.727 24–40 Kbps 20 ms 0x0E G.727 32–40 Kbps 20 ms 0x0F G.723 5.3 Kbps 30 ms 0x10 G.723 6.3 Kbps 30 ms 0x11 G.729 20 ms

See Programmable Protocol Language.
Outgoing call setup during real-time call processing on a specific channel.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
PCM and companding standard used in Europe to compress and expand the amplitude range of a signal before and after transmission. See µ-Law.
PCM and companding standard used in North America and Japan to compress and expand the amplitude range of a signal before and after transmission. See A-Law