0x0A Delay N Milliseconds

See also 0x11, Delay N Milliseconds as used in the Route Control and Outseize messages

Delay values are measured in units of 10 milliseconds. The maximum delay value is 10 seconds (0x03E8).

Used in:
Inseize Control message

ICB Type | 0x01 (Action)
ICB ID | 0x0A or 0x11
Data Length | 0x02
Data[0, 1] | Delay Value (MSB, LSB)

Outgoing call setup during real-time call processing on a specific channel.
See Information Control Block.
Most Significant Bit
Least Significant Bit