0x4C Deregister PPL Components

Used in:
Multi-Host Configure message

ICB Type | 0x02 (Data)
ICB ID | 0x4C
Data Length | Variable
Data[0-3] | Host ID
Data [4+] | PPL Component ID 1 (2 bytes)
: | :
: | PPL Component ID n (2 bytes)

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
See Information Control Block.
See Programmable Protocol Language.
A programmable software component that uses PPL state machines that can be modified with the PPL Tool.