0x060E Automatic Gain Control Parameters

Use this TLV in the Resource Create (0x0124) and Generic Card Configure (0x0122) messages to set the time constant over which gain is measured in a conference.

Byte | Description
0, 1 | Tag: 0x060E Automatic Gain Control Parameters
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Time Constant (5 ms steps) Min: 100 (0x0064) Max: 20000 (0x4E20) Default: 2000 (0x07D0)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.