0x02D5 H.245 Tunneling Configure

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

This TLV globally turn tunneling on and off. When this TLV is set to enable, the IP Signaling card accepts incoming H.323 calls with the H.245 tunneling feature.

Byte | Description
0, 1 | Tag 0x02D5
2, 3 | Length 0x0001
4-7 | Value[0] 0 - Disabled (default) 1 - Enabled

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
ITU-T standard defines a set of call control, channel setup, and codec specifications for transmitting real-time voice and video over networks that do not offer guaranteed service or quality of service.