0x4E24 Acceptance Rate

Used in:
0x1E Generic PPL ICB in PPL Request message

Byte | Description
0, 1 | Tag 0x4E24
2, 3 | Length 0x0003
4 | Value[0] ACL Level 0x01 or 0x02
5,6 | Value[1,2] Acceptance Rate - Number of calls per second for this ACL Level. MSB - Acceptance Rate LSB - Acceptance Rate

See Programmable Protocol Language.
See Information Control Block.
Most Significant Bit
Least Significant Bit