0x2C V5 ID

If this AIB is used, the user port ID must be specified in a V5 Subscriber ID ICB (0x28). In the PPL Event Indication message this AIB and the Channel (0x0D) AIB are used for the V5 Layer 3P PSTN protocol. The V5 Configure and V5 Configuration Query messages also use this AIB.

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x2C
3 | Data Length 0x02
4 | Data[0] V5 ID (MSB)
5 | Data[1] V5 ID (LSB)

See Address Information Block.
See Information Control Block.
See Programmable Protocol Language.
Public Switched Telephone Network
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
Most Significant Bit
Least Significant Bit