0x2936 SIP Tunnel Type

For all outgoing messages, this TLV enables and disables the use of tunneled data and specifies the tunneled data type.Used in:
0x0033 NPDI Universal ICB in:
Route Control message
Outseize Control message
PPL Event Request message

Byte | Description
0, 1 | Tag 0x2936
2, 3 | Length 0x0002
4-6 | Value[0-2] 0x0001 No tunneling (Default) 0x0002 CSP UPDF Tunneling 0x0004 Custom MIME Body

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.
See Programmable Protocol Language.
See Universal Protocol Data Format.