0x000A V5 C Channel Assignment

Used in:
V5 Configure message
V5 Configuration Query message

Byte | Description
0 | Tag 0x00 V5 C Channel Assignment (MSB)
1 | Tag 0x0A V5 C Channel Assignment (LSB)
2 | Length 0x00 (MSB)
3 | Length 0x06 (LSB)
4 | Type 0x01 = PG1 Primary 0x02 = PG1 Secondary 0x03 = PG#2 (Not Supported)
5 | Logical Span ID for Primary Link, MSB
6 | Logical Span ID for Primary Link, LSB
7 | Primary Physical Channel 16
8 | V5 C Channel ID 0x00 = Primary 0x01 - 0x2B = Others
| Link ID

Most Significant Bit
Least Significant Bit
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.