You are here: PPL Developer’s Guide > 6 SS7 Atomic Functions > ISUP SSC (0x0085)

ISUP SSC (0x0085)

This section documents the atomic functions associated with ISUP SSC.

Atomic Functions

AF Number | 52
Name | Send ISUP message to CPC
Type | Normal
Description | Sends message with the event specified in arg1 to CPC
Arg1 | Event
| 0 : 255
Arg2 | <Not Used>

AF Number | 53
Name | Test parameter with bitmask
Type | Test
Description | Test the parameter provided in arg1 with the bit-mask in the in arg2.
Arg1 | Parameter ID
| 0 : 255
Arg2 | Bitmask
| 0 : 255
Result | PPLevIntEVENT_1 – If Bit mask qualifies PPLevIntEVENT_0 – If it does not

AF Number | 54
Name | Store Message in buffer
Type | Normal
Description | Store the message in the MSG buffer.
Arg1 | <Not Used>
Arg2 | <Not Used>

AF Number | 55
Name | Assemble message in buffer
Type | Normal
Description | Assemble the message in MSG and SGM buffer into the MSG buffer.
Arg1 | <Not Used>
Arg2 | <Not Used>

AF Number | 56
Name | Send SGM message to L3P
Type | Normal
Description | Send the incoming Segmentation Message to L3P.
Arg1 | Event ID
| 0 : 255
Arg2 | <Not Used>

AF Number | 57
Name | Send ISUP message to L3P
Type | Normal
Description | Send the incoming ISUP message to L3P.
Arg1 | Event ID
| 0:255
Arg2 | <Not Used>

AF Number | 58
Name | Send Pass-through message to L5
Type | Normal
Description | Forward Pass through message to L5.
Arg1 | ISUP message config index
| 0 :255
Arg2 | <Not Used>

AF Number | 59
Name | Forward Incoming Message to L3P
Type | Normal
Description | Forwards Call control messages to L3P.
Arg1 | Event
| 0 : 255
Arg2 | <Not Used>

AF Number | 60
Name | Forward Message to CPC
Type | Normal
Description | This messages forwards the message to CPC without any changes to it.
Arg1 | Event
| 0: 255
Arg2 | <Not Used>

AF Number | 61
Name | Send the Segmented Message to CPC
Type | Normal
Description | The AF sends the constructed SGM message to CPC.
Arg1 | Event ID
| 0:255
Arg2 | <Not Used>

AF Number | 62
Name | Store message in SGM buffer
Type | Normal
Description | Store incoming SGM message in SGM buffer.
Arg1 | <Not Used>
Arg2 | <Not Used>

AF Number | 63
Name | Test COT check flag in CPC
Type | Normal
Description | Test COT wait before RFS flag in CPC.
Arg1 | <Not Used>
Arg2 | <Not Used>

See Integrated Services Digital Network User Part.
See Atomic Function.
In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.
See Request For Service.