0x01C8 Protocol Type

Use this TLV to specify the protocol used by the TLVs in the VoIP Protocol Configure and VoIP Protocol Query messages.

Used in:
0x1E Generic PPL ICB in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x01C8
2, 3 | Length 0x0001
4 | Value[0] 0x04 SIP 0x05 H.323 0x06 RFC 2833

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Programmable Protocol Language.
See Information Control Block.
Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.
ITU-T standard defines a set of call control, channel setup, and codec specifications for transmitting real-time voice and video over networks that do not offer guaranteed service or quality of service.