0x01D0 Gateway Mode

Use this TLV to configure an IP Network Interface Series 2 card to be in Gateway Mode or Normal Mode.

Important! This TLV is addressed to a card, and therefore cannot be combined in a message with any other TLVs.

Used in:
Resource Attribute Configure message

Byte | Description
0, 1 | Tag: Gateway Mode (0x01D0)
2, 3 | Length: 0x0001
4 | Value: Setting 0x01 Gateway Mode (Non-port Consuming Mode) 0x02 Normal Mode (Port Consuming Mode)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A device that translates calls between an IP network and another network, typically the PSTN.
The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."