You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > EXS Node Configure 0x007F

EXS Node Configure 0x007F

SwitchKit Name

NodeConfig

Type

EXS API and SwitchKit API message

Description

EXS Node Configure 0x007F

Use this message to configure entities in a node.

Sent by

Host

SwitchKit Code

Configuration

NodeConfig (

Node = integer,

Entity = integer,

DataLen = integer,

Data = byte array);

C Structure

typedef struct {

unsigned short Entity;

UBYTE DataLen;

UBYTE Data[250];

} XL_NodeConfig;

C Structure Response

typedef struct {

unsigned short Status;

unsigned short Entity;

UBYTE DataLength;

UBYTE Data[248];

} XL_NodeConfigAck;

C++ Class

class XLC_NodeConfig : public XLC_OutboundMessage {

public:

unsigned short getEntity() const;

void setEntity(unsigned short x);

UBYTE getDataLen() const;

void setDataLen(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

C++ Class Response

class XLC_NodeConfigAck : public XLC_AcknowledgeMessage {

public:

unsigned short getStatus() const;

void setStatus(unsigned short x);

unsigned short getEntity() const;

void setEntity(unsigned short x);

UBYTE getDataLength() const;

void setDataLength(UBYTE x);

const UBYTE *getData() const;

UBYTE *getData();

void setData(UBYTE *x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0xNNNN)
3, 4 | Message Type (0x007F) | 3, 4 | Message Type (0x007F)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
8, 9 | Entity 0x0001 Number of Timeslots 0x0002 Reserved 0x0003 Number of EXNET Connect Channels 0x0004 Clock Master 0x0005 Master on Multiple Ring Configure 0x0006 CTNETREF/PCI H.100 | 8, 9 | Status MSB, LSB
10, 11 | Entity
10 | Data Length | 12 | Data Length
11 | Data The meaning of this field depends on the value of the Entity field. 0x0001 Number of Timeslots Data Length: 0x02 The value of this word-length field represents the number of timeslots assigned for CSP Conferencing. The valid entry for this field is as follows: Data[0,1] 0xFFFF Assign all unused timeslots 0x0002 Unused Important: There must be at least 256 unlicensed timeslots available to allocate any timeslots. | 13 | Data The meaning of these fields depends on the value of the Entity field in the message. 0x0001 Number of Timeslots Valid entries for these fields based on the Entity field value 0x01 are as follows: Data Length: 0x02 Data[0,1] Number of Timeslots Allocated for CSP Conferencing Conferencing (MSB, LSB) 0x02 Unused
|  | : | Checksum
| 0x03 Number of EXNET Connect Channels Data Length: 0x03 Data[0, 1] Span (MSB, LSB) All spans 0xFFFF Data[2] Number of Channels 0x18 - 24 (T1) 0x20 - 32 (E1) Note: You must de-assign spans before modifying the number of channels per span. 0x04 Clock Master Data Length: 0x03 Data[0] Slot Number Data[1] Bus Master 0x00 Not SCbus clock master/H.100 Slave to clock A 0x01 Become SCbus clock master/H.100 primary clock master driving clock A 0x02 H.100 secondary clock master driving clock A 0x03 H.100 slave to clock B 0x04 H.100 primary clock master driving clock B 0x05 H.100 secondary clock master driving clock B Data[2] Speed 0x00 4 MHz 0x01 2 MHz (Reserved) 0x02 8 MHz Example Data[2] corresponds to the local bus speed. Value 0x00 corresponds to SCSA compatibility mode speed for PCI/H.100 card.
| 0x05 Master on Multiple Ring Configure |  |
| Indicates whether or not a node is allowed to become the EXNET® Master of multiple rings. Data Length: 0x01 Data[0] Master on Multiple Ring Flag 0x01 Allow this node to be Master on more than one ring simultaneously. 0x00 Do not allow this node to be Master on more than one ring simultaneously. (Default)
| 0x06 CTNETREF Data[0] Slot Number
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
Peripheral Component Interconnect
Most Significant Bit
Least Significant Bit
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
See Signal Computing System Architecture.
Message delimiter (SS7 bit pattern - 01111110)