0x9045 Signaling Gateway Process

Used in:
NGA Configure message

Byte | Description
0, 1 | Tag 0x9045
2, 3 | Length 0x0007
4,5 | Value[0,1] Port Number
6 | Value [2] Number of IP Addresses
7-10 | Value [3-6] IP Addresses

The point in the Excel platform where a DS0 connects to a network. Also known as a "socket."
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.