0x1A Call Type

Call Types:

0x0001 L3P Controlled

0x0002 Host Controlled

If the value of the Call Type field is 0x0001, the remaining data fields Data[2] through Data[n], represent the digits of the called party number.

The called party digits are noted in ASCII/IA5 format. For example, the digit "5" is indicated as 0x35.

If the value of the Call Type field is 0x0002, data fields Data[2] through Data[n] are not included in the ICB.

Used in:
Route Control message
Outseize Control message

ICB Type | 0x02 (Data)
ICB ID | 0x1A
Data Length | Variable
Data[0, 1] | Call Type MSB, LSB
Data[2] | Called Party Digit
Data[3] | Called Party Digit
Data[4] | Called Party Digit

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
American Standard Code for Information Interchange
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.
Most Significant Bit
Least Significant Bit