0x0100 RTP Payload Type (IPN Series 3)

Used in:
0x1E and 0x001E Generic PPL ICBs in:
Route Control message
Outseize Control message
Resource Attribute Query message
Resource Attribute Configure message

Byte | Description
Profile 4
0, 1 | Tag 0x0100 RTP Payload Type
2, 3 | Length 0x0001
4 | Value[0] Payload Type Basic Packet Rate 0x00 G.711 A-Law 5 ms 0x01 G.711 µ-Law (Default) 5 ms
Profile 5
0, 1 | Tag 0x0100 RTP Payload Type
2, 3 | Length 0x0001
4 | Value[0] Payload Type Basic Packet Rate 0x00 G.711 A-Law 5 ms 0x01 G.711 µ-Law (Default) 5 ms 0x02 G.726 16 Kbps 5 ms 0x03 G.726 24 Kbps 5 ms 0x04 G.726 32 Kbps 5 ms 0x05 G.726 40 Kbps 5 ms 0x0F G.723 5.3 Kbps 30 ms 0x10 G.723 6.3 Kbps 30 ms 0x11 G.729 10 ms

See Programmable Protocol Language.
Outgoing call setup during real-time call processing on a specific channel.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.
PCM and companding standard used in Europe to compress and expand the amplitude range of a signal before and after transmission. See µ-Law.
PCM and companding standard used in North America and Japan to compress and expand the amplitude range of a signal before and after transmission. See A-Law