0x12 SS7 Parameters

Used in:
Channel Release Request, Channel Released With Data, Connect With Data, Release Channel with Data, Route Control, Outseize Control, PPL Event Indication, PPL Event Request messages.

ICB Type | 0x02 (Data)
ICB ID | 0x12
Data Length | Variable
ISUP Message ID | See the list of supported ANSI ISUP message types, in the API Developer’s Guide: Common Channel Signaling.
Data[0] | Number of Parameters
Data[1] | Parameter 1 Type
Data[2] | Parameter 1 Length
Data[3] | Parameter 1 Data[0] (consult ANSI or ITU-TS recommendations for data)
Data[:] | Parameter n Type
Data[:] | Parameter n Length
Data[:] | Parameter n Data[0] (consult ANSI or ITU-TS recommendations for data)

Outgoing call setup during real-time call processing on a specific channel.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
See Integrated Services Digital Network User Part.
American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.
International Telecommunications Union (UN)