You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > CPA Tone Patterns

CPA Tone Patterns

The default tone patterns for call progress analysis appear in Default tone patterns for call progress analysis. To modify or create new patterns, use the CPA Pattern Configure message. Click on the pattern name to see the default parameters (web-based documentation only).

Table 8-13 Default tone patterns for call progress analysis

Value | CPA Tone Pattern
0x01 | Ringback
0x02 | Double Ringback
0x03 | Busy
0x04 | Reorder
0x05 | PBX intercept
0x06 | SIT Intercept
0x07 | Vacant Code
0x08 | Reorder LEC
0x09 | No Circuit LED
0x0A | Reorder Carrier
0x0B | No Circuit Carrier
0x0C | PBX Dialtone
0x0D | Standard Dial Tone
0x0E | CPC Detection
0x13 | Fax
0x14 | 2100Hz

See Private Branch Exchange.