You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Distant End Release Mode 0x00B8

Distant End Release Mode 0x00B8

SwitchKit Name

DistantReleaseConfig

Type

EXS API and SwitchKit API message

Description

Distant End Release Mode 0x00B8

This message sets a channel’s distant end release mode, which determines whether the distant end is released or parked when the connection is terminated.

Sent by

Host

SwitchKit Code

Configuration

DistantReleaseConfig (

Node = integer,

Range = StartSpan:StartChan - EndSpan:EndChan,

ReleaseMode = integer);

C Structure

typedef struct {

unsigned short StartSpan;

UBYTE StartChannel;

unsigned short EndSpan;

UBYTE EndChannel;

UBYTE ReleaseMode;

} XL_DistantReleaseConfig;

C++ Class

class XLC_DistantReleaseConfig : public XLC_ChanRangeMessage {

public:

unsigned short getStartSpan() const;

void setStartSpan(unsigned short x);

UBYTE getStartChannel() const;

void setStartChannel(UBYTE x);

unsigned short getEndSpan() const;

void setEndSpan(unsigned short x);

UBYTE getEndChannel() const;

void setEndChannel(UBYTE x);

UBYTE getReleaseMode() const;

void setReleaseMode(UBYTE x);

};

EXS API Hex Format

MESSAGE (White) | RESPONSE (Gray)
Byte | Field Description | Byte | Field Description
0 | Frame (0xFE) | 0 | Frame (0xFE)
1, 2 | Length (0xNNNN) | 1, 2 | Length (0x0007)
3, 4 | Message Type (0x00B8) | 3, 4 | Message Type (0x00B8)
5 | Reserved (0x00) | 5 | Reserved (0x00)
6 | Sequence Number | 6 | Same Sequence Number
7 | Logical Node ID | 7 | Logical Node ID
: | AIB Address Method 0x01 - Range of AEs | 8, 9 | Status MSB, LSB
Number of AEs to follow 0x02
0x0D Channel (Starting) 0x0D Channel (Ending)
: | Release Mode 0x01 Park 0x02 Release (Default) | 10 | Checksum
: | Checksum

A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
A group of data bits in a specific format, with a flag at each end to indicate the beginning and the end of the frame.
See Address Information Block.
Most Significant Bit
Least Significant Bit