0xFF PPL General Purpose Register Data

Used in:
PPL Event Indication message
PPL Event Request message

ICB Type | 0x02 (Data)
ICB ID | 0xFF
Data Length | Variable
Data[0-7] | Event Data

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.