You are here: Changes from Previous Release > 1 Changes from Previous Releases > Changes in Release 8.4.1 Service Pack 17

Changes in Release 8.4.1 Service Pack 17

FR5721

This feature allows the CPA Receiver to report only the 2100Hz tone event and ignore all other results. This capability makes the screen more user friendly for maintenance and monitoring.

Refer to the following updates to the API documentation:

• DSP Service Request message (0x00BD) - Service Type 0x05 Tone Detector

In PPL, a condition that, when met, drives a state machine (PPL Component) from one state to another, by invoking an associated Primitive. In PPL files, an Event is marked by an arrow and text.
Digital Signal Processor