0x0116 Channel Service TLV

Indicates whether the connection being established will be switched through the CSP or will bypass the CSP.

For VoIP calls, if this TLV is not present in one of the messages listed below, a switched CSP connection is created.

For non-VoIP calls, this TLV is ignored and an CSP switched connection is created.

Used in:
0x1E Generic PPL ICB in:
PPL Event Request message
Connect with Data message

Byte | Description
0, 1 | Tag 0x0116
2, 3 | Length 0x0001
4, 5 | Value[0-1] Bearer Service Mode: 0x0000 - Bearer-switched through the CSP which implies a physical span channel. 0x0001 - Bearer-free. The CSP is bypassed which implies a virtual span channel.

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
See Programmable Protocol Language.
See Information Control Block.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.