0x01EC Media Inactivity Detection Timer

Use this TLV to create a timer for monitoring the incoming RTCP packets (VDAC-ONE) or UPD packets (IPN Series 2) at a per module or a per channel basis to detect possible media inactivity occurrence. When this timer is enabled for a particular channel, if the configured timer value has elapsed and no RTCP/UPD packets are received, then this timer will expire and generate a PPL Event Indication with Event ID of 0x08 to alert the host of a possible media inactivity detection. RTCP/UPD must be supported by remote endpoints for this TLV to work.

Used in:
0x1E Generic PPL ICB in:
Resource Attribute Configure message
Route Control message
Outseize Control message (not for SIP or H.323)

Byte | Description
0, 1 | Tag 0x01EC
2, 3 | Length 0x0004
4, 5 | Value[0,1] 0x0000
6, 7 | RTP Timer Timeout Value (2 Bytes - 10 ms increments) 0x00 - 0xFFFF ms. 0x00 is the default, and it means that the timer is disabled. Any other value automatically enables the timer to that value.

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Real-Time Transport Control Protocol.
See Programmable Protocol Language.
See Information Control Block.
Outgoing call setup during real-time call processing on a specific channel.
Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.
ITU-T standard defines a set of call control, channel setup, and codec specifications for transmitting real-time voice and video over networks that do not offer guaranteed service or quality of service.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.