You are here: CSP Developer’s Guide: Common Channel Signaling > 7 SS7 PPL Information > L3P CIC (0x000F)

L3P CIC (0x000F)

In this section:

Purpose

L3P CIC Configuration Bytes (ITU)

L3P CIC Config Bytes with Offset Values (ITU)

L3P CIC PPL Event Indications (ITU)

L3P CIC PPL Event Requests (ITU)

L3P CIC PPL Timers (ITU)

L3P CIC PPL Configuration Bytes (ANSI)

L3P CIC PPL Event Indications (ANSI)

L3P CIC PPL Timers (ANSI)