L3P SSUTR2 PPL Event Indications

Event ID | Event
--- | ---
0x28 | Received IFG
0x29 | Received MSA/MSS
0x2B | Received NRP
0x2D | Received DEG
0x2E | Received ACF
0x2F | Received RIU
0x30 | Received call unsuccessful
0x31 | Received RAU
0x32 | Outgoing (Remote) maintenance block indication
0x35 | Outgoing (Remote) maintenance unblock indication
0x38 | Incoming (Local) maintenance block request successfully completed
0x39 | Incoming (Local) maintenance block request unsuccessful
0x3A | Incoming (Local) maintenance unblock request successfully completed
0x3B | Incoming (Local) maintenance unblock request unsuccessful
0x40 | Incoming (Local) maintenance blocking clear indication
0x44 | L5 reset/ group reset successful
0x45 | L5 reset/ group reset unsuccessful
0x64 | TUP protocol violation
0x65 | Resources not available for continuity check
0x0259 | Received end to end message MUU/MCE
0x025A | Received CHT
0x025B | Received ITX
0x025C | Received TAX
0x025D | Received TXA
0x025E | System error block request successfully completed
0x025F | System error block request unsuccessful
0x0260 | System error unblock request successfully completed
0x0261 | System error unblock request unsuccessful
0x0262 | Outgoing block unsuccessful (Already blocked)
0x0263 | Outgoing unblock unsuccessful (Not blocked)
0x0264 | BLOF operation unsuccessful
0x0265 | BLOF clear unsuccessful

Telephone User Part