0x0750 Dial Pulse Detection Parameters

Use this TLV in the Generic Card Configure and Generic Card Query messages.

Byte | Description
0, 1 | Tag: 0x0750 - Dial Pulse Detection Parameters
2, 3 | Length: 0x000A
4, 5 | Value[0, 1]: Low Threshold Level - The sample level required to be below in order to declare sample as a Low Signal Default - 0x1388 (5000)
6, 7 | Value[2, 3]: Low Threshold Count - The number of consecutive low samples to be considered a post Dial Pulse Low Default - 0x0011 (17)
8, 9 | Value[4, 5]: Peak Threshold - The sample value required for a signal to be declared a Dial Pulse Peak Default - 0x36B0 (14000)
10, 11 | Value[6, 7]: Maximum Transition Count - The maximum low to high transition time (samples). For a peak to be declared, the ramp time has to be less than this number of samples. Default - 0x7530 (30000)
12, 13 | Value[8, 9]: Settle By Count: Number of consecutive samples that the signal must be below the low threshold to declare the signal as a dial pulse. Default - 0x0190 (400)

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.