0x05DC File Management Configuration

Use this TLV to specify the type of server to be used for recorded voice files. This TLV is used in the Generic Card Configure message and in the response to the Generic Card Query message for the DSP Series 2 card.

Byte | Description
0, 1 | Tag 0x05DC File Management Configuration
2, 3 | Length 0x0001
4 | Value[0] 0x01 NFS

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Digital Signal Processor