DASS2/DPNSS

Comp. ID | Comp. Name | PPL Assign | PPL Audit Config | PPL Audit Query | PPL Config | PPL Data Query | PPL Event Request | PPL Timer Config
--- | --- | --- | --- | --- | --- | --- | --- | ---
0x000D | DASS2/DPNSS L3P CC | Channel, B (0x0D) | N/A | Channel, B (0x0D)
0x000E | DASS2/DPNSS L3P D Channel | Channel, D only (0x0D) | Channel, D only (0x0D)
0x0051 | DPNSS L3P VCC | Channel, B (0x0D) | Channel, B (0x0D)

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
Data channel. One of two fundamental components of an ISDN interface, it provides a path (16Kbps for BRI, 64Kbps for PRI) for carrying control signals and call data in a packet-switched mode.