You are here: CSP Developer’s Guide: Overview > 8 DSP Series 2 Cards Product Description > Default Tone Patterns for CPA Detection

Default Tone Patterns for CPA Detection

All of the tones supported by the CSP for are shown in Tones supported by the CSP. The group of tone IDs may use up to 16 frequencies. A pattern is formed when the tones below are played at specific intervals.

Table 8-12 Tones supported by the CSP

Tone ID | Frequency Count | Frequency 0 (Hz) | Frequency 1 (Hz)
--- | --- | --- | ---
0x00 | 1 | 0 |
0x01 | 2 | 350 | 440
0x02 | 2 | 440 | 480
0x03 | 1 | 440 |
0x04 | 1 | 480 |
0x05 | 2 | 480 | 620
0x06 | 1 | 620 |
0x07 | 1 | 914 |
0x08 | 1 | 985 |
0x09 | 1 | 1371 |
0x0A | 1 | 1429 |
0x0B | 1 | 1777 |
0x0C | 1 | 2000 |
0x0D | 1 | 1700 |
0x0E | 1 | 2100 |
0x0F | 1 | 425 |
0x10 | 1 | 500 |
0x11 | 1 | 1100 |

Hertz