PPL Event Indications

Event ID | Event
--- | ---
0x01F5 | ACI Received
0x01F6 | SAM Received
0x01F7 | FAM Received
0x01F8 | Undefined Message Received
0x01F9 | Call Connected Indication
0x01FA | SND Received
0x01FB | CNG Received
0x01FC | CNA Received
0x01FD | RAM Received
0x01FE | SEM Received
0x01FF | SAD Received
0x0200 | CFN Received
0x0201 | Error, timer expired sending ACI request
0x0202 | Error, timer expired sending SASUI request
0x0203 | ASUI Received
0x0204 | SASUI Received
0x0205 | IAM Received
0x0206 | IFAM Received
0x0207 | ACM Received
0x0208 | TCM Received
0x0209 | SOO Received
0x020A | ANS Received
0x020B | CLR Received
0x020C | RAN Received
0x020D | REL Received
0x020E | CCF Received
0x020F | OLM Received
0x0210 | BLA Received
0x0211 | UBA Received
0x0212 | BLO Received
0x0213 | UBL Received
0x0214 | Circuit already Blocked
0x0215 | Circuit Not Blocked
0x0216 | Remote Block Indication, Circuit already Blocked
0x0217 | Remote Unblock Indication, Circuit not Blocked
0x0218 | Error Timer Expired, Sending CNA
0x0219 | Network ANS received before ACM
0x021A | SSM Received
0x021B | SER Received
0x021C | ECM Received
0x021D | CFC Received
0x021E | OOR Received
0x021F | HLR Received
0x0220 | SIM Received
0x0221 | SUS Received
0x0222 | RES Received
0x0223 | SWAP Received

L3P BT IUP to Host--Access Denied Message

Whenever L3P BT IUP sends an Access Denied message to Call Control, two arguments are included: Reason and Call Status.

The table below shows the Reasons that may be sent to the host with Access Denied messages. When placing an outbound call, L3P BT IUP may determine that the call cannot be completed. When this occurs, an Access Denied message is sent to the host with the Reason fields encoded.

Reasons for Access Denied Messages

:

Reason | Description
--- | ---
0x1B | Outseize Failure, No ACK
0x1C | Outseize Failure, Glare detected.
0x25 | Invalid Encoding Format
0x59 | Outseize Failure, Call Blocked.

Call Status Values:

Call Status | Description
--- | ---
0x00 | Call Inactive
0x01 | Call Active. Call is already established on this channel.

Random Access Memory
See Recorded Announcements.
Blocking Acknowldgment message
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Setting up, monitoring, and tearing down calls.
Outgoing call setup during real-time call processing on a specific channel.
Positive acknowledgment to a message