0x16 SS7 Protocol Violation Data

Used in:
PPL Event Indication message
PPL Event Request message

ICB Type | 0x02 (Data)
ICB ID | 0x16
Data Length | 0x05
Data[0, 1] | PPL Component ID
Data[2] | Error Type NOTE: Entries marked with a dagger (†) report the ISUP message type only and do not report an ISUP parameter. 0x01† Unrecognized Message Type 0x02 Unrecognized Parameter ID 0x03 Minimum Parameter Length Violation 0x04 Maximum Parameter Length Violation 0x05† Corrupt Parameter Data 0x06† Mandatory Parameters Missing 0x07 Range Field of Range/Status Parameter is zero
Data[3] | ISUP Message ID To see a list of supported ANSI ISUP message types, refer to the SS7 Chapter in the API Developer’s Guide: Common Channel Signaling
Data[4] | ISUP Parameter ID See the API Developer’s Guide: CCS. If the value of the Error Type field is marked with a †, the value of this field is 0x00.

See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Information Control Block.
A programmable software component that uses PPL state machines that can be modified with the PPL Tool.
See Integrated Services Digital Network User Part.
American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
See Signaling System Number Seven.
CCS. Network architecture using SS7 protocol for the exchange of information between telecommunications nodes and networks on an out-of-band basis.
See Common Channel Signaling.