You are here: CSP Hardware Product Descriptions > 3 Line Cards > Dialogic® T-ONE 100 Ohm Standby I/O Card - EXSTIO1300/EXSTIO1300R

Dialogic® T-ONE 100 Ohm Standby I/O Card - EXS-TIO-1300/EXS-TIO-1300R

Description

The Dialogic® T-ONE 100 Ohm Standby I/O card is used in conjunction with a Redundant I/O card to deliver N + 1 redundancy to all system line cards. If an active line card fails, the affected data stream is rerouted to a Standby card. The software enables you to automate the switch-over process or control it from a remote location.The Standby I/O card has no external connections. All of its features and functionality are internal to the system.

Active or Switchover Mode

The Standby I/O card LED indicates whether the card is in Active or Switchover Mode. A red light indicates the Standby card is active (Switchover Mode). A green light indicates that the card is not active (Standby Mode).

Placement

The card resides in the rear card slot of a CSP 2090, CSP 2110 or CSP 2040 chassis.

Configuration Information

The part number, serial number, model number, and revision are located on the back of the board.

Specifications

The T-ONE 100 Ohm Standby I/O card is designed to the following electrical, physical and environmental specifications.

Electrical | Specification
--- | ---
Supply Voltage, Vcc | 5.00V
Supply Current, Vcc @ 5.0V | 0.95A (typical)

Physical | Specification
--- | ---
Height | 318.5 mm (12.54 in.)
Depth | 105.2 mm (4.14 in)
Width | 19.7 mm (0.775 in.)

Environmental | Specification
--- | ---
Temperature - Storage | -40~C to 70~C (-40~F to 158~F)
Temperature - Operation | 0~C to 50~C (32~F to 122~F)
Temperature Shock - Storage | -40~C to 70~C to -40~C (-40~F to 158~F to -40~F) @ 5~C/min.
Temperature Shock - Operation | 0~C to 50~C (32~F to 122~F) @ 10~C/min.
Humidity - Operating | 5% to 85%
Altitude | Up to 4000 m (13,123 ft.)

Related Products

The products related to the T-ONE 100 Ohm Standby I/O card are listed below.

Product | Model No. | RoHS Model No.
--- | --- | ---
T-ONE Card | EXS-T1C-1160 | EXS-T1C-1160R
T-ONE 100 Ohm I/O Card | EXS-TIO-1000 | EXS-TIO-1000R
T-ONE 100 Ohm Red I/O Card | EXS-TIO-1200 | EXS-TIO-1200R

Front and Side Views

The front view shows the Status LED.

Controls and Indicators

The table below describes the LED as shown in the front view.

LED | Color/Status | Description
--- | --- | ---
Status | Green/Standby Mode | Standby card is not active
Red/Active Mode | Standby card is active

Flow of Voice and Data in Active and Switchover Modes

The table below describes the Active and Switchover Modes.

Symbol | Mode | Description
--- | --- | ---
1 | Active | Voice and data flow from the T1 span into the T-ONE 120 Ohm Redundant I/O card where they are switched to the system bus and routed to the active line card.
2 | Switchover | Voice and data on the T-ONE 120 Ohm Redundant I/O card are switched to the Redundant I/O bus and routed to the T-ONE 120 Ohm Standby I/O card where they are switched to the system bus and routed to the Standby line card.

Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)