You are here: CSP API Reference > 1 EXS & SwitchKit API Messages > Numerical List of EXS API Messages

Numerical List of EXS API Messages

0x0000 Connect 0x0000

0x0001 Channel Connection Status Query 0x0001

0x0002 Version Request 0x0002

0x0003 Connect With Pad 0x0003

0x0005 Connect With Data 0x0005

0x0006 Synchronization Priority List Query 0x0081

0x0007 Card Population Query 0x0007

0x0008 Release Channel 0x0008

0x000A Service State Configure 0x000A

0x000B Reset Configuration 0x000B

0x000C Clear System Software 0x000C

0x000D Subrate Connection Management 0x000D

0x000F DS3 Configure/Query 0x000F

0x0010 Assign Logical Node ID 0x0010

0x0011 Trunk Type Configure 0x0011

0x0012 Filter/Timer Configure 0x0012

0x0013 Start Dial Configure 0x0013

0x0014 Transmit Signaling Configure 0x0014

0x0015 Receive Signaling Configure 0x0015

0x0016 Flash Timing Configure 0x0016

0x0017 Connect Wait 0x0017

0x0018 Busy Out 0x0018

0x0019 J1 Span Configure 0x0019

0x001A Cross Connect Channel 0x001A

0x001B Cross Disconnect Channel 0x001B

0x001C Cross Connect Span 0x001C

0x001D Cross Disconnect Span 0x001D

0x001E Disconnect Tone Pattern 0x001E

0x0020 Outpulse Digits 0x0020

0x0021 Local End Release Mode Configure 0x0021

0x0023 Standby Line Card Configure 0x0023

0x0024 Line Card Switchover 0x0024

0x0028 Inpulsing Parameters Configure 0x0028

0x0029 Inseize Instruction List Configure 0x0029

0x002A Outseize Instruction List Configure 0x002A

0x002B Inseize Control 0x002B

0x002C Outseize Control 0x002C

0x002D Request For Service With Data 0x002D

0x002E Call Processing Event 0x002E

0x002F Connect Tone Pattern 0x002F

0x0030 Transmit Cadence Pattern Configure 0x0030

0x0031 Tone Configure 0x0031

0x0034 Call Progress Analysis Result 0x0034

0x0036 Release Channel With Data 0x0036

0x0037 Channel Release Request 0x0037

0x003A TFTP Manage 0x003A

0x003D Generic Event Logger Configure/Query 0x003D

0x0040 Request For Service 0x0040

0x0042 DS0 Status Change 0x0042

0x0043 PPL Event Indication 0x0043

0x0044 PPL Event Request 0x0044

0x0045 Diagnostics Indication 0x0045

0x0046 Generic Report 0x0046

0x0047 CPC Detection 0x0047

0x0049 Channel Released 0x0049

0x004A Loop Timing Configure 0x004A

0x004B Conference Create 0x004B

0x004C Conference Delete Request 0x004C

0x004D Conference Deleted 0x004D

0x004E Connect To Conference 0x004E

0x004F Connect One-Way To Conference 0x004F

0x0050 Connect One-Way Forced 0x0050

0x0052 Recorded Announcement Download Initiate 0x0052

0x0053 Recorded Announcement Download 0x0053

0x0054 Recorded Announcement Delete 0x0054

0x0055 Recorded Announcement Connect 0x0055

0x0056 Recorded Announcement Disconnect 0x0056

0x0057 Recorded Announcement Query 0x0057

0x0058 Recorded Announcement Report 0x0058

0x0059 Transmit Cadence Pattern Query 0x0059

0x005A Tone Query 0x005A

0x005B CCS Redundancy Configure 0x005B

0x005C SS7 Signaling Stack Configure 0x005C

0x005D SS7 Signaling Link Set Configure 0x005D

0x005E SS7 Signaling Link Configure 0x005E

0x005F SS7 Signaling Route Configure 0x005F

0x0060 ISDN Interface Configure 0x0060

0x0062 ISDN Terminal Configure 0x0062

0x0063 ISDN Query 0x0063

0x0064 SS7 Signaling Link Set Query 0x0064

0x0065 SS7 Signaling Link Query 0x0065

0x0066 SS7 Signaling Route Query 0x0066

0x0067 SS7 CIC Query 0x0067

0x0068 SS7 ISUP Message Query 0x0068

0x0069 Channel Released With Data 0x0069

0x006A SS7 CIC Configure 0x006A

0x006B SS7 ISUP Message Format Configure 0x006B

0x006C CCS Redundancy Query 0x006C

0x006D SS7 Signaling Stack Query 0x006D

0x006E Assign EXS Host/Slave 0x006E

0x006F Node Status Query 0x006F

0x0070 Node Status Report 0x0070

0x0071 Ring Status Query 0x0071

0x0072 Ring Status Report 0x0072

0x0073 CCS Redundancy Report 0x0073

0x0074 EXNET Ring Configure 0x0074

0x0077 SS7 SCCP/TCAP Configure 0x0077

0x0078 SS7 SCCP/TCAP Query 0x0078

0x0079 Product License Download 0x0079

0x007A Product License Query 0x007A

0x007B V5 Configure 0x007B

0x007C V5 Configuration Query 0x007C

0x007D Matrix Configure 0x007D

0x007E EXS Node Configuration Query 0x007E

0x007F EXS Node Configure 0x007F

0x0080 Channel Parameter Query 0x0080

0x0081 Synchronization Priority List Query 0x0081

0x0082 System Log Query 0x0082

0x0083 Card Status Query 0x0083

0x0084 Span Status Query 0x0084

0x0085 T1 Span Query 0x0085

0x0086 Fault Log Query 0x0086

0x0087 Call Control Instructions Query 0x0087

0x0089 Inpulsing Parameters Query 0x0089

0x008A Call Progress Analysis Configuration Query 0x008A

0x008E System Resource Usage Query 0x008E

0x008F SS7 TUP Message Format Configure 0x008F

0x0090 SS7 TUP Message Query 0x0090

0x0092 SNMP Configure 0x0092

0x0091 Loop Back Configure/Query 0x0091

0x0097 Matrix Query 0x0097

0x009B Download Begin BRecord 0x009B

0x009C Download BRecord 0x009C

0x009D Reset Matrix 0x009D

0x009E Poll Request 0x009E

0x009F Poll Interval Configure 0x009F

0x00A1 Become Active 0x00A1

0x00A2 Download Begin SRecord 0x00A2

0x00A3 Download SRecord 0x00A3

0x00A4 Download Complete 0x00A4

0x00A6 Card Status Report 0x00A6

0x00A8 Assign Logical Span ID 0x00A8

0x00A9 T1 Span Configure 0x00A9

0x00AB Poll 0x00AB

0x00AF System Configuration 0x00AF

0x00B2 Call Progress Analysis Pattern Configure 0x00B2

0x00B3 Call Progress Analysis Class Configure 0x00B3

0x00B4 System Configuration Query 0x00B4

0x00B5 Time Set 0x00B5

0x00B8 Distant End Release Mode 0x00B8

0x00B9 Alarm 0x00B9

0x00BA Generate Call Processing Event 0x00BA

0x00BB Answer Supervision Mode Configure 0x00BB

0x00BC Collect Digit String 0x00BC

0x00BD DSP Service Request 0x00BD

0x00BE DSP Service Cancel 0x00BE

0x00BF Park Channel 0x00BF

0x00C0 DSP SIMM Configure 0x00C0

0x00C1 Alarm Cleared 0x00C1

0x00C4 D Channel Assign 0x00C4

0x00C5 D Channel De-assign 0x00C5

0x00C6 D Channel Facility List Query 0x00CB

0x00C8 B Channel Configure 0x00C8

0x00CA B Channel Query 0x00CA

0x00CB D Channel Facility List Query 0x00CB

0x00CD Span Filter Configure 0x00CD

0x00CE Span Filter Query 0x00CE

0x00CF PPL Timer Configure 0x00CF

0x00D0 Tag Configuration 0x00D0

0x00D1 PPL Assign 0x00D1

0x00D2 PPL Transmit Signal Configure 0x00D2

0x00D3 Busy Out Flag Configure 0x00D3

0x00D4 PPL Create 0x00D4

0x00D5 PPL Table Download Initiate 0x00D5

0x00D6 PPL Table Download 0x00D6

0x00D7 PPL Configure 0x00D7

0x00D8 E1 Span Configure 0x00D8

0x00D9 PCM Encoding Format Configure 0x00D9

0x00DA PPL Delete 0x00DA

0x00DB E1 Span Query 0x00DB

0x00DC PPL Audit Configure 0x00DC

0x00DD PPL Audit Query 0x00DD

0x00DE PPL Data Query 0x00DE

0x00DF PPL Protocol Query 0x00DF

0x00E0 Virtual Card Configure 0x00E0

0x00E2 Virtual Span Control 0x00E2

0x00E3 Resource Attribute Configure 0x00E3

0x00E4 Resource Attribute Query 0x00E4

0x00E5 Matrix Status Report 0x00E5

0x00E6 IP Address Query 0x00E6

0x00E7 IP Address Configure 0x00E7

0x00E8 Route Control 0x00E8

0x00E9 Multi-Host Configure 0x00E9

0x00EA SS7 CLLI Configure 0x00EA

0x00EB SS7 CLLI Query 0x00EB

0x00EE VoIP Protocol Configure 0x00EE

0x00EF VoIP Protocol Query 0x00EF

0x00F0 IP Socket Configure 0x00F0

0x00F1 IP Socket Query 0x00F1

0x00F2 IP Socket Status Report 0x00F2

0x00FB ARP Cache Report 0x00FB

0x00FC ARP Cache Query 0x00FC

0x0100 IP Signaling Series 3 Card Configure 0x0100

0x0101 IP Signaling Series 3 Card Query 0x0101

0x0102 Recorded Announcement File System Query 0x0102

0x0103 Recorded Announcement File System Defragment 0x0103

0x0104 IP Signaling Series 3 Card Host Poll 0x0104

0x0105 IP Signaling Series 3 Card Status Report 0x0105

0x0107 Reset IP Signaling Series 3 Card 0x0107

0x0108 Clear IP Signaling Series 3 Card 0x0108

0x0117 Recorded Announcement Single Delete 0x0117

0x0118 Recorded Announcement File System Convert 0x0118

0x0119 Recorded Announcement File System Report 0x0119

0x011A DSP Cache Modify 0x011A

0x011B Play File Start 0x011B

0x011C Play File Modify 0x011C

0x011D Play File Stop 0x011D

0x011E Record File Start 0x011E

0x011F Record File Modify 0x011F

0x0120 Record File Stop 0x0120

0x0121 Statistics Query 0x0121

0x0122 Generic Card Configure 0x0122

0x0123 Generic Card Query 0x0123

0x0124 Resource Create 0x0124

0x0125 Resource Modify 0x0125

0x0126 Resource Delete 0x0126

0x0127 Resource Connect 0x0127

0x0128 Resource Disconnect

0x0129 Resource Delete Indication

0x012C Resource Query

0x0130 NGA Configure 0x0130

0x0131 NGA Configure Query 0x0131

0x0160 NGA Service Configure 0x0160

0x0161 NGA Service Query 0x0161

0x0162 NGA State Query 0x0162

0x0163 NGA State Notify 0x0163

The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.
Quick depress and release of the phone plunger of a handset to signal the PBX or Centrex of instructions to follow (e.g., Call Transfer).
Range of channels provided by T1 or E1 transmission service. A physical span is a group of channels taking up a single physical wire. A logical span is a group of channels taking up less than a single logical wire, or carried over more than one physical wire.
Outgoing call setup during real-time call processing on a specific channel.
RFS. A Status Message indicating that some entity is requesting service from the Excel platform.
Pattern of tones and silence, such as a busy signal.
See Programmable Protocol Language.
A condition that, when met, drives a state machine from one state to another. A condition that drives a Component out of its current state by invoking an associated primitive.
See Common Channel Signaling.
See Signaling System Number Seven.
Link that connects to the same node
See Integrated Services Digital Network.
See Circuit Identification Codes.
See Integrated Services Digital Network User Part.
A computer, attached to the Excel platform through an RS-232 or Ethernet link, from which you run the telecommunications application that controls the Excel platform.
Excel's open architecture, proprietary, 1.3 Gbps fiber optic network using a packet-based protocol.
See Transaction Capability Application Part.
Digital communications link - voice, data, and video at a 1.544 Mbps rate (24 64 Kbps channels)
Setting up, monitoring, and tearing down calls.
Telephone User Part
Digital Signal Processor
Data channel. One of two fundamental components of an ISDN interface, it provides a path (16Kbps for BRI, 64Kbps for PRI) for carrying control signals and call data in a packet-switched mode.
Bearer channel, 64Kbps (ISDN) The channel that carries the actual payload (as opposed to D-channels, which carry signaling data that helps route the payload).
Message delimiter (SS7 bit pattern - 01111110)
A digital communications link - voice, data, and video at a 2.048 Mbps rate; 30B/2D or 31B/1D (ISDN); non-North American version of T1.
See Pulse Code Modulation.
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).