0x2D V5 ID, Link ID

The V5 ID, Link ID address type is used for Link blocking and unblocking.

Byte | AIB Field Description
--- | ---
2 | Address Element: 0x2D
3 | Data Length 0x03
4 | Data[0] V5 ID (MSB)
5 | Data[1] V5 ID (LSB)
6 | Data[2] Link ID

See Address Information Block.
The information in an AIB that follows the header, down to the data field. An AIB can have one or more Address Elements. AEs correspond to Span, Channel, and SS7 Link.
Most Significant Bit
Least Significant Bit