0x060F Conference Failure Behavior

Use this TLV in the Resource Connect (0x0127) and Generic Card Configure messages (0x0122) to choose whether a channel is purged or parked when a conference fails.

Byte | Description
0, 1 | Tag: 0x060F Conference Failure Behavior
2, 3 | Length: 0x0002
4, 5 | Value[0, 1]: Conference Failure Behavior 0x0000 - Purge Channel (Default) 0x0001 - Park Channel

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.