L3 BT IUP CPC Configuration Bytes

Byte | Definition | Value
0x01 | Network Configuration Bit Number Description | 0=Controlled Network (default) 1=Controlling Network
0x02 | Confusion Message Qualifier value Whenever CPC sends the Confusion message this byte will be used to setup the message qualifier byte. | 0 (default)
0x03 | Incoming Congestion Control. | 0=Enabled (default) 1=Disabled
0x04 | Release Procedures | 0 = Both way Procedures 1 = Disabled
0x05 | Unidirectional Customer Location (i.e. Outgoing Network Location) Used for Idle Release Procedures | 0 = Other End 1 = This End
0x06 | Bearer Release Outgoing Initiated, Subsequent to sending the third release processing procedure | 0 =Assume Circuit is Blocked 1 = Repeatedly send a Release upon expiry of TO-12 2 = Assume circuit is Idle, ready to accept another call.