SCCP SCRC Configuration Bytes

Byte | Description | Value
0x01 | SCCP Flow Control=Indicates if SCCP should perform remote SCCP Status Check when routing on GT. | 0x00- No (ANSI default) 0x01=Yes (ITU default)
0x02 | Point Code Congestion Status=Indicates if SCCP should check the APC Congestion Status and not send a message to a congested point code. | 0x00- No (ITU default) 0x01=Yes (ANSI default)
0x03 | Supports the GR-246 congestion handling option. When enabled, the CSP routes the message based on the point code congestion level during GTT. | 0x00 = Disabled (default) 0x01 = Enabled

American National Standards Institute. ANSI administers and coordinates the U.S. voluntary standardization and conformity assessment system for the
telecommunications industry. More details on these standards may be
viewed at www.ansi.org.
International Telecommunications Union (UN)
A number that addresses a node in a SS7 network.