0x2762 Date and Time
(Interworking Only)

Used in:
0x0033 NPDI Universal ICB

Byte | Description
0, 1 | Tag 0x2762
2, 3 | Length Variable
4, 5 | Value[0] Year AD MSB, LSB
6 | Value[1] Month (1-12) 1- January : 12 - December
7 | Value[2] Day 1-31
8 | Value[3] Hour 0-24
9 | Value[4] Minute 0-59
10 | Value[5] Seconds 0-59
11, 12 | Value[6] Millisecond 0-999
13 | Value[7] Zone Information 0x00 GMT 0x01 EST (USA & Canada) 0x02 CST (USA & Canada) 0x03 MST (USA & Canada) 0x04 PST (USA & Canada) 0x05 Atlantic Time (Canada) 0x06 Newfoundland Time (Canada) 0x07 Indian Time 0xF0 to 0xFD User Defined 0xFF Not set or Unknown All the other values are reserved.
14 | Value[8] Daylight Savings Considerations 0x00 DST not in effect 0x01 DST in effect 0x02 DST not used at all in this time zone. 0xF0 to 0xFD User Defined 0xFF Not set or Unknown All the other values are reserved.

Network Protocol Data Intelligence. Also called “Interworking,” it is a software product that operates within Excel’s Call Control (Layer 4) and Services (Layer 5) call processing layers. NPDI is meant to enhance Excel’s call processing product offering by allowing call processing layers (specifically Layers 4 and 5) to perform advanced analysis, generation, and conversion of Network Signaling (NS) Layer 3 information.
See Information Control Block.
Most Significant Bit
Least Significant Bit
A collection of newer network components, such as terminals, gateways, gatekeepers, and multipoint control units (MCU) that interoperate with other standards-compliant endpoints and networks by virtue of an H.323 gateway. The collection of all these network components, which are managed by a single Gatekeeper, is referred to as an H.323 Zone. A zone includes at least one terminal, and can include gateways or multipoint control units (MCUs), or LAN segments connected using routers. A zone has only one gatekeeper.