You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Loopback Options on a DS3 or T-ONE Card

Loopback Options on a DS3 or T-ONE Card

Accessing the loopback options

To access the loopback options on a DS3 card, right click the card in the node view. Select one of the loopback-related options. For the DS3 card, the following loopback options are available in CSA Query Loopback Status
Enable Local Loopback
Disable Local Loopback
Disable Local Loopback and Bring into service
Request Remote Loopback
Cancel Remote Loopback

For the T-ONE, the following loopback are available:

Query Loopback Status
Enable Local Loopback
Disable Local Loopback
Disable Local Loopback and Bring into service

See Converged Services Administrator.
A type of diagnostic test in which the transmitted signal is returned to the sending device after passing through a data communications link or network.