0x01C5 Fax Type Enable

If the fax type is set to Disable, then the fax will go through as a voice call. Therefore, the fax transmission might not be successful.

Used in:
0x1E Generic PPL ICB in:
Resource Attribute Query message
Resource Attribute Configure message

Byte | Description
0, 1 | Tag 0x01C5 Fax Type Enable
2, 3 | Length 0x0001
4 | Value[0] ONE of the following: 0x00 Disable (Default) - RTP not changed. 0x01 Enable Relay 0x02 Enable Bypass

See Programmable Protocol Language.
See Information Control Block.
Real-Time Transport Protocol. Supports transport of real-time data like interactive voice and video over packet-switched networks.