0x026B Use SIP Max Retransmissions BYE

Use this TLV to specify the maximum retransmissions for a BYE request (any request other than INVITE). The default value is 0x0B.

Used in:
VoIP Protocol Configure message
VoIP Protocol Query message

Byte | Description
0, 1 | Tag 0x026B
2, 3 | Length 0x0001
4 | Value[0] Maximum Transmissions

Tag-Length-Value block. A standardized block that allows data to inserted in a standard way into API messages.
Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).