0x0065 Physical VoIP Channel

Indicates to the router to hunt a physical VoIP channel.

Used in:
PPL Table Download message
0x1E Generic PPL ICB in Route Control message

Byte | Description
0, 1 | Tag 0x0065
2, 3 | Length 0x0002
4,5 | Value[0-1] 0x0000

Voice over Internet Protocol. The delivery of voice information in digital form in discrete packets rather than in the traditional circuit-committed protocols of the public-switched telephone network (PSTN).
See Programmable Protocol Language.
See Information Control Block.