You are here: SwitchKit® Development Environment - CSA User’s Guide > 7 System Provisioning and Monitoring > Querying SIP Configuration

Querying SIP Configuration

This procedure describes how to query the SIP configuration.

Before you begin

Make sure that the LLC and SwitchManager are running. For information on running the LLC and SwitchManager refer to the SwitchKit documentation.

Querying procedure

Follow the steps below to query the SIP configuration.

1 Right-click in the node view window (outside the card slots) and select Query SIP Configuration or select the menu Provisioning® SIP®Query SIP Configuration. The next window opens:

2 Click Show Advanced to see the current SIP configuration.The SIP Advanced window opens. See the screen shot on the next page.

Session-Initiation Protocol. A signaling protocol used for establishing sessions in an IP network. A session could be a simple, two-way telephone call, or it could be a collaborative multi-media conference session.