L3P BCC PPL Timers

When specifying new timer values, remember that all PPL Timers are specified in 10 ms increments. For example, a PPL timer for 4 seconds is specified as 4000 (decimal, 400 x 10 ms = 4 seconds), which is the hexadecimal value of (0x190).

Timer ID | Description | Value (default)
--- | --- | ---
0x01 | Layer 4 Router Response Wait | 4 seconds
0x02 | Layer 3 Audit Complete Wait | 4 seconds
0x03 | Layer 3 Audit Complete | 4 seconds

See Programmable Protocol Language.
Call processing layer of the CSP.
Protocol layer of the CSP.