You are here: CSP Developer’s Guide: Overview > 7 Configuring and Using Resources on the DSP Series 2 Cards > DSP Configuration API Message Summary

DSP Configuration API Message Summary

Introduction

The following table shows the API message used for DSP configuration.

GENERAL DSP CONFIGURATION
Tasks | Options/Notes | API Message(s)
Assign Function Types | See Function Types | DSP SIMM Configure
Configure NFS | File Management Server Address Vocabulary Index File NFS User Group ID NFS Poll Retries | Generic Card Configure
Configure Overload Alarm Thresholds | See Configuring Overload Management
Assign IP Address | Required for NFS | IP Address Configure
Bring DSP In Service |  | Service State Configure
FUNCTION-SPECIFIC CONFIGURATION
Tasks | Options/Notes | API Message(s)
Conferencing
Configure Card-level Conferencing Parameters | Output Gain Control Noise Gating Echo Suppression Auto. Gain Control Failure Behavior | Generic Card Configure
Record Files
Record Files | Gain File Event Descriptor Beep Tone Parameters Initial Silence Timer Final Silence Timer Max. Record Timer Dual Chan. Rec. Option Silence Threshold Append or Replace | Record File Start Record File Stop
Modify Recording | Modify Gain Pause Resume | Record File Modify
Tones
If required, modify default tones and Call Progress Analysis Pattern/Class. | See Customizing Tones. | Call Progress Analysis Pattern Configure Call Progress Analysis Class Configure Tone Configure Inseize Instruction List Configure
Implementing DSP Resources
Conferencing | See Conferencing. | Resource Create Resource Connect Resource Modify Resource Disconnect
Play Files | See Playing a File. | DSP Service Request DSP Service Cancel Play File Start Play File Modify Play File Stop
Record Temporary Files | See Recording Files. | Record File Start
Tones | See Tones. | DSP Service Request DSP Service Cancel Connect Tone Pattern Disconnect Tone Pattern

Digital Signal Processor
Internet Protocol. Part of the TCP/IP family of protocols used to route messages and tracks the addresses of nodes.
A 32-bit address, used in IP routing, which includes a Network address identifier assigned by a central authority and a Host ID (an end station identifier assigned by a LAN administrator).
The condition of a component at a given instant. The current "context" of a PPL object, such as Idle, Seizing, Answered. In PPL files, a State is represented by a circle.